|  |  |
| --- | --- |
| **Part Number** | **JS1640F2-W** |
| Center frequency kHz | 40.0±1.0 |
| Output sound pressure dB@30cm/10V sine wave | ≥105 |
| Receive sensitivity dB / v / μbar | ≥-82 |
| -6dB Directivity deg. | 75±10 |
| Ringing Time ms | ≤0.8 |
| Capacitance pf @ 120Hz 25℃ | 2000±10% |
| Input voltage Vp-p | 140 |
| Operating Temperature℃ | -40~+80 |
| Storage Temperature℃ | -40~+85 |
| Materials of the case | Aluminum |
| Type of the terminal | Connector |
| Length of the lead wire mm | 2500±50 |

Parameter: